Course: High Performance Computing Lab

Practical No 1

PRN:21510055

Name: Siddhesh S Kitkaru

Batch: B3

Title: Introduction to OpenMP

Problem Statement 1 – Demonstrate Installation and Running of OpenMP code in C

Recommended Linux based System:

Following steps are for windows:

OpenMP – Open Multi-Processing is an API that supports multi-platform shared-memory multiprocessing programming in C, C++ and Fortran on multiple OS. OpenMP uses a portable, scalable model that gives programmers a simple and flexible interface for developing parallel applications for platforms ranging from the standard desktop computer to the supercomputer.

To set up OpenMP,

We need to first install C, C++ compiler if not already done. This is possible through the MinGW Installer.  
Reference: Article on GCC and G++ installer ([Link](https://www.scaler.com/topics/c/c-compiler-for-windows/))

Note: Also install `mingw32-pthreads-w32` package.

Then, to run a program in OpenMP, we have to pass a flag `-fopenmp`.

Example:

To run a basic Hello World,

*#include* <stdio.h>

*#include* <omp.h>

*int* main(*void*)

{

*#pragma* *omp* *parallel*


    printf("Hello, world.\n");

*return* 0;

}

gcc -fopenmp test.c -o hello

.\hello.exe




Problem Statement 2 – Print ‘Hello, World’ in Sequential and Parallel in OpenMP

We first ask the user for number of threads – OpenMP allows to set the threads at runtime. Then, we print the Hello, World in sequential – number of times of threads count and then run the code in parallel in each thread.

Code snapshot:



Output snapshot:




Analysis:


GitHub Link: <https://github.com/Sid-1164/HPC_lab/tree/main/prac%201>

Problem statement 3: Calculate theoretical FLOPS of your system on which you are running the above codes.

Elaborate the parameters and show calculation.

=>





based on above information :

No of Flops= No of Core \* ClockSpeed \* IPC \* 10\*\*9

No of Core = 6

Clock Speed = 2.60 GHz

IPC = This value varies depending on the workload and CPU architecture. For modern CPUs like the Intel Core i7-10750H, IPC is generally around 4 for floating-point operations, but this is an approximation.

ANS = 62.4 GFLOPS